// EOS
shift = 0 				// EOS Address Shift
writefreq = 1 			// Device Write Frequency
readfreq = 1 			// Device Reading Frequency
silent = false 			// Device Sleep Mode (for Local Controllers) [true/false]

// IEC60870
writefreq = 1 			// Device Write Frequency
readfreq = 1 			// Device Reading Frequency
spontaneousonly = false		// Use Spontaneous Data Transfer Only Mode [true/false]
usesendmessagequeue = false 	// Use Message Queue Feature [true/false]
silent = false 			// Device Sleep Mode (for Local Controllers) [true/false]
connreset = 0                  		// Device Periodic Connection Refresh Time (Seconds) [=0 Feature Off]
connreset = 0                  		// Device Periodic Connection Refresh Time (Seconds) [=0 Feature Off]
asducountreset=false                              // Connection Periodic Reset If No ASDU Packet Received in 5 Minutes

// DNP3
writefreq = 1 			// Device Write Frequency
readfreq = 1 			// Device Reading Frequency
spontaneousonly = false 		// Use Spontaneous Data Transfer Only Mode [true/false]
localaddress = 2 			// Local Address
remoteaddress = 1 			// Remote Address
scaninterval = 60000 		// Scan Interval
silent = false 			// Device Sleep Mode (for Local Controllers) [true/false]

//IEC61850
writefreq = 1 			// Device Write Frequency
readfreq = 1 			// Device Reading Frequency
datasetmode = false 		// Dataset Mode [true/false]
silent = false 			// Device Sleep Mode (for Local Controllers) [true/false]
origin = station_control		// Originator Category (not_supported, bay_control, station_control, remote_control, automatic_bay, automatic_station, automatic_remote, maintenance, process) 

// MODBUS
shift = 0				// Modbus Address Shift
writefreq = 1			// Device Write Frequency
readfreq = 1 			// Device Reading Frequency
transit = 0 			// Constant Transaction ID
masswrite = false 			// Mass Write [true/false]
lockinterval = 1000 			// Transaction Lock Timeout
exitcontext = true 			// Stop Lock Wait on Timeout [true/false]
locktype = none 			// Action Lock Type [none/read/write/both]
silent = false 			// Device Sleep Mode (for Local Controllers) [true/false]

//OPC
writefreq = 1 			// Device Write Frequency
readfreq = 1 			// Device Reading Frequency
silent = false 			// Device Sleep Mode (for Local Controllers) [true/false]
connreset = 0                  		 // Device Periodic Connection Refresh Time (Seconds) [=0 Feature Off]

//S7PLC
rack = 0 				// Rack Number
slot = 0 				// Slot Number
writefreq = 1 			// Device Write Frequency
readfreq = 1 			// Device Reading Frequency
silent = false 			// Device Sleep Mode (for Local Controllers) [true/false]

// LIVEDB
tablename = ANLIK_DURUM 		// Live Table Name
valuecolname = DEGER 		// VALUE Column Name in Live Table
datecolname = TARIH 		// TIME Column Name in Live Table
veriidcolname = VERI_ID 		// DATA IDENTIFICATION ID Column Name in Live Table
sid = 				// Database System Identifier (SID)
silent = false 			// Device Sleep Mode (for Local Controllers) [true/false]

// TXT
seperator = 			// Character Used As Separator Between Data
usetimestamp = false 		// Use Timestamp [true/false]
writefile = build-force.txt 		// File Name For Data Write
readfile = build-simulation.txt		 // File Name For Data Read

// MSMQ
seperator = 			// Character Used As Separator Between Data
usetimestamp = false 		// Use Timestamp [true/false]
writefile = build-force.txt 		// File Name For Data Write
readfile = build-simulation.txt		 // File Name For Data Read